**Instructions of suction type Hand-print printer**


1. Rack screen: put in the screen and tighten the screws.



1. Adjust the height of the screen,and pay attention the level.



1. Adjust the print position:loosen the side screws to adjust the position of the printing platform front,back,left,and right.



1. Pour ink on the screen to start printing.