**Finecause - Characteristics of Contact Lens and Rubber Pads**

Finecause - Characteristics of Contact Lens and Rubber Pads

|  |  |
| --- | --- |
| 1.Finecause provides fast and accurate new molding process. New pads will be |  |
| completed within 7 days after confirmation of the drawings. completed. |
| 膠頭 |
| 2.Negative pressure value reaches 2 TOLL and above when |
| 佳因 膠頭 |
| Finecause Rubber Pad 　　　　　　Other Rubber pad |
| 3.We developed the silicone with characters that suits the best for 　contact lens ink and with even color.  4.We inspect every single pad produced for its straightness. 檢驗垂直度 |
|  |
|  |
| 5.After pad de-molding process, there is no deckle edge for the center hole. 膠頭 |  |
|  |  |
| 6.Quality control of the adhesion for rubber pad and metal aluminum base. |
|  |
| 7.Strict quality control of the Rubber Pad cleanliness. |
|  |
| 8.Leading techniques and quality in the industry with competitive prices. |
|  |