**Contact lens rubber pad**

* Finecause provides fast and accurate new style mold opening. After confirming the drawing , 10 days a new rubber pad can finished for testing.
* The negative pressure value of the rubber pad is more than -2TOLL(referring to the pressure unit), and there are no bubbles in the profile.
* Developed the characteristics of silicone that are especially suitable for contact lens inks, evenly colored.
* Check the straightness of each rubber pad before leaving the factory.
* After the rubber pad is demoulded, the inner hole has no burrs.
* The hardness machine test the softness and hardness of each rubber pad.
* Rubber pad and metal aluminum seat join adhesion quality control.
* The quality control of rubber pad appearance cleanliness is strict.